**Interior: Suggested Maximum Deductions:*****05/2018***

***Evaluate each item for Authenticity and Condition***

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| CATEGORY | Max Ded | MINOR | SIGNIFICANT | MAJOR | MAX DEDUCTION |
| HEADLINER  Visors | 2 | Stain or wear greater than patina -1/2  Small rips or tears -1/2  NOR Craftsmanship -1/2 | Not original design -1  Significant wear, rips or tears -1 | Reproduction materials  NOR in appearance, design orworkmanship -1 | No headliner or Visors -2  NOR appearance, design  & workmanship -2 |
| UPHOLSTERY  Seats, Console, Door & Shelf Panels | 4 | Stain or wear greater than patina -1/2  NOR craftsmanship -1/2  Small rips or tears -1/2  Period seatbelts, neat alarm, safety,   communications equipment, -0 | Significant wear, rips or tears-1  Poor reproduction materials -1  NOR in appearance, design **or** workmanship -1  Obtrusive accessories -1 | Non-Ferrari seats -2  NOR Upholstery -2 | Material, design & craftsmanship NOR on  several components -4 |
| CARPET  Pedals & Shifter | 3 | Stain or wear greater than patina -1/2  NOR style stitching/binding -1/2  NOR pattern/form pad or boot -1/2  NORfinishes or craftsmanship -1/2 | Missing heel pad or top boot -1 | Poor repo materials -1  NOR in appearance, design   or workmanship -1 | No carpet -3 or  NOR appearance, design   & workmanship -3 |
| DASHBOARD:  Instruments;  Mirror | 3 | Small scratches/wear -1/2  Faded faces -1/2  NOR style paint or finish -1/2 | Significant scratches/wear -1  Holes or additional components -1 | Modified dashboard -2 | Dashboard & instruments   NOR / significant   deterioration -3 |
| STEERING Wheel,   Horn; Signals | 2 | Small nicks or scratches -1/2 | Significant wear or scratches -1  Horn INOP -1 | Incorrect Ferrari wheel -1 | Incorrect wheel -2  (Non Ferrari/aftermarket) |
| TRIM  EMBLEMS | 2 | Poor plating or condition -1/2  Incorrect screws -1/2 | Each one NOR appearance or   missing -1 | X | Two missing or two NOR in   appearance or design -2 |
| TRUNK Carpet,  Paint, Decals   Hardware | 2 | Stains or wear greater than patina -1/2  Small rips or tears -1/2  NOR style hardware or plating **-**1/2 | NOR style carpet or paint -1  Significant rips or tears -1 | X | No carpet and/or paint -2  NOR materials, finish, style  & craftsmanship -2 |
| TOOLS Spare,   Manual, Crank,   Jack, etc. | 4 | NOR wheel, tire, manual **or** pouch -1/2  NOR jack and tire tools for type -1/2  No window crank **or** trouble light -1/2  No warranty book, wipe rag -0 | Several missing tools or bag -1/2  No tools and bag -1  No manual and pouch -1 | No spare and wheel -1  No jack & changing tools -1  No puncture repair kit -1 | No tools, manuals, spare, jack and puncture repair -4 |
| WINDOW  Operation | 2 | Each sticky window -1/2 | Each window INOP -1 | |  | | --- | | Sunroof or convertible top (electric) INOP -1 | | Maximum -2 |
| INSTRUMENT / FAULT MODE   Operation | 3 | Clock, radio, or dash light INOP -1/2 Hood, trunk, glovebox light INOP -1/2 | Each instrument INOP -1 Heater fan, AC INOP -1  Each fault mode indicator INOP -1 | Several INOP -2 | Maximum -3 |
| EXTERIOR LIGHT  Operation | 4 | Non-critical side marker INOP -1/2  License plate light INOP -1/2 | Each significant light INOP -1 | X | Maximum -4 |

X=Does Not Apply International Advisory Council for Preservation of the Ferrari Automobile (IAC/PFA) **©** 1994, 1999,